Author: Gregg Maroney

HUDSON-TERRAPLANE
OPERATING INSTRUCTIONS
Read Carefully Before Driving Your Car

IGNITION SWITCH -Turn key to right to turn on ignition.
MANUAL CHOKE KNOB (TERRAPLANE DELUX AND COMMERCIAL MODEL ONLY) - pull out when starting engine. Push in gradually as engine warms up.
Clutch pedal - depress manually before turning on ignition switch when starting engine. When car is equipped with Hill Hold depress manually to keep breaks applied on upgrade.
Starter button - depress after turning on ignition and depressing clutch pedal.
Automatic clutch control knob - pushed in permits operation of clutch automatically. Pulled out permits manual operation.
Light switch knob - extreme left is off position, turn to first clockwise position for parking lights and full clockwise position for bright lights.
Light switch foot control -
Locker box knob -